### Answer Key

|  |  |  |  |
| --- | --- | --- | --- |
| Question | MEWB No. | Answer | Illustration |
| 1. | 1011. | b |  |

1. Permanent centrifugal pump shaft damage due to erosion, corrosion, and wear at the stuffing box is usually prevented by \_\_\_\_\_\_\_\_\_\_.
   1. wearing rings
   2. renewable sleeves
   3. a hardened sprayed metal coating
   4. internally flooded lantern rings

### Illustrations